Max. power input 1400 W

• Nominal power input 1200 W

• Suction power 250 W

• Noise level: < 77 dB

• Aluminium telescopic tube

• Washable inflow microfilter

• Washable outflow microfilter

• Automatic cord winding

• Electronically controlled suction power

• Universal floor nozzle with an extensible brush