**Max. power input 1400 W**

**• Nominal power input 1200 W**

**• Suction power 250 W**

**• Noise level: < 77 dB**

**• Aluminium telescopic tube**

**• Washable inflow microfilter**

**• Washable outflow microfilter**

**• Automatic cord winding**

**• Electronically controlled suction power**

**• Universal floor nozzle with an extensible brush**